airCentric™Multi Tilt [air-MT]

|  |  |
| --- | --- |
| Backrest   * 5" Patented Back Height Adjustment System * Front Upholstered Dual Curve Backrest (19"w x 24"h) * Plastic Back Cap with Airflow Vents * Proprietary Airflow Molded Polyurethane Foam and Structure   Arms   * [Click here](http://ergocentric.com/resource/arms) to view options   Seat   * Tailored Upholstery on Seat Pan (20”w x 19”d) * Proprietary Airflow Molded Polyurethane Foam and Structure   **Options:**   * Extra Long Non-Airflow Seat (20”w x 21”d) [XLS] * Small Non-Airflow Seat (18.5”w x 17”d) [SS] * Triple Density Foam (adds ¼” to seat width and depth) (Not available on airCentric seat options) [TDF] * Standard Non-Airflow Seat (20”w x 19”d) [LS] * airCentric Plus Size Seat (22”w x 19”d) [ACPS]] * airCentric Small Seat (18.5”w x 17”d) [ACSS]   Multi Tilt Mechanism   * Infinite Forward Tilt Lock Out * Infinite Lock Free Float * Back Angle Adjustment * Adjustable Spring Tension * 2.5” Depth Adjustable Seat Slider   Pneumatic Lift (Seat Height)   * 125 mm Pneumatic Lift (16.5" – 21.5")   **Options:**   * 80 mm Pneumatic Lift (only available with 26” Glass Reinforced Nylon Base) (15.75”-18.75”) [80mm] * 100 mm Pneumatic Lift (16”-19.5”) [100mm] * 140 mm Pneumatic Lift (17.5”-23”) [140mm] | Base/Glides/Casters   * 25" Glass Reinforced Nylon High Profile Base * 5 Dual Wheel Nylon Carpet Casters   **Options:**   * 2 ¼” Glides [2G] * Chrome Accent Casters [CAC] * 26” Polished Aluminum Base [PB] * Single Wheel Casters [SW] * Single Wheel Urethane Casters [SWU] * Urethane Casters [UC] * 26” Glass Reinforced Nylon Base [26NB]   Additional Options   * 24 Hour Multi Tilt Mechanism (Warranted for 24 Hour Use up to a weight of 280 lbs.) [24MT] * Air Lumbar [AL] * Memory Foam Seat (Not Available on airCentric seat options) [EA] * Adjustable Headrest [AHR] * Cal. 133 [Cal133] |