High Wipe Down Bench Stool[HI-WDBS]

|  |  |
| --- | --- |
| Frame* 14 Gauge, 7/8" Steel Tube Frame
* Height (Polyurethane Seat Options) 31"
* Chrome footring provides additional leg support (height) 12"
* Non-slip and non-making glides (black) work with all floor surfaces
 | Additional Options* ergoCentric+Guard Sealed Seat (includes under seat pan) [EGUSS]
* Cal. 133 [Cal133]
* Anti Static (Available in fabric and vinyl only) [ANTISTATIC]
* Class 100 Cleanroom (only available in vinyl) [CRPACK]
 |