High Wipe Down Bench Stool[HI-WDBS]

|  |  |
| --- | --- |
| Frame   * 14 Gauge, 7/8" Steel Tube Frame * Height (Polyurethane Seat Options) 31" * Chrome footring provides additional leg support (height) 12" * Non-slip and non-making glides (black) work with all floor surfaces | Additional Options   * ergoCentric+Guard Sealed Seat (includes under seat pan) [EGUSS] * Cal. 133 [Cal133] * Anti Static (Available in fabric and vinyl only) [ANTISTATIC] * Class 100 Cleanroom (only available in vinyl) [CRPACK] |