Ergo 2F ESD 200™Tilt [ERGO 2F 200 ESD TILT FR]

|  |  |
| --- | --- |
| Backrest   * Fully Upholstered Dual Curve Backrest * 17" wide by 19" high   Arms   * [Click here](http://ergocentric.com/resource/arms) to view options   Seat   * High Resilient Polyurethane Foam * Seat Pan 20" wide by 19" deep   **Options:**   * Memory Foam Seat [EA] * ESD Small seat - 18.5"W x 17"D [ESDSS] * Triple Density Foam Seat (Adds 1/4" to seat width and depth) [TDF]   3 Lever Tilt Mechanism   * Back Angle Adjustment * Back Height Adjustment * Seat Tilt   Pneumatic Lift (Seat Height)   * 200 mm ESD pneumatic lift (20.5"-27.5")   **Options:**   * 267 mm ESD pneumatic lift (23"-33") [267mm] | Base/Glides/Casters   * 1 1/4"ESD Glides * 26" High Pressure Die Cast Polished Aluminum Base * Surface to Ground Resistance 105 - 109 OHMS * 20" Diameter Height Adjustable Footring (for use as a foot rest only)   **Options:**   * Urethane ESD Casters (adds 1" to seat height) [EUC] * Lock-on ESD Urethane Casters (adds 1" to seat height) [ELON] * Lock-off ESD Urethane Casters (adds 1" to seat height) [ELOF]   Upholstery   * Chair in vinyl or fabric   **Options:**   * Back Trim [BT] * Class 100 Cleanroom (only available in vinyl) [CRPACK] |

