Ergo 2F ESD 200™Tilt [ERGO 2F 200 ESD TILT FR]

|  |  |
| --- | --- |
| Backrest* Fully Upholstered Dual Curve Backrest
* 17" wide by 19" high

Arms* [Click here](http://ergocentric.com/resource/arms) to view options

Seat* High Resilient Polyurethane Foam
* Seat Pan 20" wide by 19" deep

**Options:*** Memory Foam Seat [EA]
* ESD Small seat - 18.5"W x 17"D [ESDSS]
* Triple Density Foam Seat (Adds 1/4" to seat width and depth) [TDF]

3 Lever Tilt Mechanism* Back Angle Adjustment
* Back Height Adjustment
* Seat Tilt

Pneumatic Lift (Seat Height)* 200 mm ESD pneumatic lift (20.5"-27.5")

**Options:*** 267 mm ESD pneumatic lift (23"-33") [267mm]
 | Base/Glides/Casters* 1 1/4"ESD Glides
* 26" High Pressure Die Cast Polished Aluminum Base
* Surface to Ground Resistance 105 - 109 OHMS
* 20" Diameter Height Adjustable Footring (for use as a foot rest only)

**Options:*** Urethane ESD Casters (adds 1" to seat height) [EUC]
* Lock-on ESD Urethane Casters (adds 1" to seat height) [ELON]
* Lock-off ESD Urethane Casters (adds 1" to seat height) [ELOF]

Upholstery* Chair in vinyl or fabric

**Options:*** Back Trim [BT]
* Class 100 Cleanroom (only available in vinyl) [CRPACK]
 |

