Ergo C 200™Standard [ERGO C 200 STANDARD FR (PU)]

|  |  |
| --- | --- |
| Backrest* Dual Curve Polyurethane Backrest
* 15" wide by 13" high

Arms* [Click here](http://ergocentric.com/resource/arms) to view options

Seat* Polyurethane Foam
* Seat Pan 19" wide by 18" deep

**Options:*** -Raised pattern design for both seat and backrest reduces slippage for additional safety. Backrest has a handle for easy maneuvering of the chair [RP]

Standard Mechanism* Back Angle Adjustment
* Back Height Adjustment
* Back Pivot

Pneumatic Lift (Seat Height)* 200 mm pneumatic lift (18.5"-25.5")

**Options:*** 267 mm pneumatic lift (21"-31") [267mm]
 | Base/Glides/Casters* 1 1/4" Glides
* 26" Glass Reinforced Nylon Base
* 20" Diameter Height Adjustable Footring (for use as a foot rest only)

**Options:*** 2 1/4" Glides (adds 1" to seat height) [2G]
* Single Wheel Urethane Casters (adds 1" to seat height) [SWU]
* Nylon Casters (adds 1" to seat height) [NC]
* Urethane Casters (adds 1" to seat height) [UC]
* Lock-on Urethane Casters (adds 1" to seat height) [LON]
* Single Wheel Casters (adds 1" to seat height) [SW]
* Lock-off Urethane Casters (adds 1" to seat height) [LOF]

Upholstery* Available in vinyl, fabric or ergoCentric+Guard

Additional Options* Back Trim [BT]
* Cal. 133 [Cal133]
* Anti Static (Available in fabric and vinyl only) [ANTISTATIC]
* Class 100 Cleanroom (only available in vinyl) [CRPACK]
 |

