Ergo C 200™Standard [ERGO C 200 STANDARD FR (PU)]

|  |  |
| --- | --- |
| Backrest   * Dual Curve Polyurethane Backrest * 15" wide by 13" high   Arms   * [Click here](http://ergocentric.com/resource/arms) to view options   Seat   * Polyurethane Foam * Seat Pan 19" wide by 18" deep   **Options:**   * -Raised pattern design for both seat and backrest reduces slippage for additional safety. Backrest has a handle for easy maneuvering of the chair [RP]   Standard Mechanism   * Back Angle Adjustment * Back Height Adjustment * Back Pivot   Pneumatic Lift (Seat Height)   * 200 mm pneumatic lift (18.5"-25.5")   **Options:**   * 267 mm pneumatic lift (21"-31") [267mm] | Base/Glides/Casters   * 1 1/4" Glides * 26" Glass Reinforced Nylon Base * 20" Diameter Height Adjustable Footring (for use as a foot rest only)   **Options:**   * 2 1/4" Glides (adds 1" to seat height) [2G] * Single Wheel Urethane Casters (adds 1" to seat height) [SWU] * Nylon Casters (adds 1" to seat height) [NC] * Urethane Casters (adds 1" to seat height) [UC] * Lock-on Urethane Casters (adds 1" to seat height) [LON] * Single Wheel Casters (adds 1" to seat height) [SW] * Lock-off Urethane Casters (adds 1" to seat height) [LOF]   Upholstery   * Available in vinyl, fabric or ergoCentric+Guard   Additional Options   * Back Trim [BT] * Cal. 133 [Cal133] * Anti Static  (Available in fabric  and vinyl only)  [ANTISTATIC] * Class 100 Cleanroom  (only available in vinyl)  [CRPACK] |

