Ergo C 200™Tilt [ERGO C ESD 200 Tilt FR (PU)]

|  |  |
| --- | --- |
| Backrest* 12" wide by 16.25" high
* Back handle for easy maneuvering of chair
* Dual curve ESD Polyurethane
* Raised pattern reduces slippage for additional safety

Arms* [Click here](http://ergocentric.com/resource/arms) to view options

Seat* ESD Polyurethane with waterfall curve
* Raised pattern reduces slippage for additional safety
* Seat Pan 17.75" wide by 17" deep

Tilt C ESD Mechanism* Back Angle Adjustment
* Back Height Adjustment
* Back Pivot
* Seat Tilt

Pneumatic Lift (Seat Height)* 200 mm ESD pneumatic lift (18.5"-25.5")

**Options:*** 267 mm ESD pneumatic lift (21"-31") [267mmESD]
 | Base/Glides/Casters* 26" High Pressure Die Cast Polished Aluminum Base
* Surface to Ground Resistance 105 - 109 OHMS
* 2 1/4" ESD Glides
* 20" Diameter Height Adjustable Footring (for use as a foot rest only)

**Options:*** Urethane ESD Casters (adds 1" to seat height) [EUC]
* - Lock-on ESD Urethane Casters (adds 1" to seat height) [ELON]
* - Lock-off ESD Urethane Casters (adds 1" to seat height) [ELOF]
 |

