Ergo C 200™Tilt [ERGO C ESD 200 Tilt FR (PU)]

|  |  |
| --- | --- |
| Backrest   * 12" wide by 16.25" high * Back handle for easy maneuvering of chair * Dual curve ESD Polyurethane * Raised pattern reduces slippage for additional safety   Arms   * [Click here](http://ergocentric.com/resource/arms) to view options   Seat   * ESD Polyurethane with waterfall curve * Raised pattern reduces slippage for additional safety * Seat Pan 17.75" wide by 17" deep   Tilt C ESD Mechanism   * Back Angle Adjustment * Back Height Adjustment * Back Pivot * Seat Tilt   Pneumatic Lift (Seat Height)   * 200 mm ESD pneumatic lift (18.5"-25.5")   **Options:**   * 267 mm ESD pneumatic lift (21"-31") [267mmESD] | Base/Glides/Casters   * 26" High Pressure Die Cast Polished Aluminum Base * Surface to Ground Resistance 105 - 109 OHMS * 2 1/4" ESD Glides * 20" Diameter Height Adjustable Footring (for use as a foot rest only)   **Options:**   * Urethane ESD Casters (adds 1" to seat height) [EUC] * - Lock-on ESD Urethane Casters (adds 1" to seat height) [ELON] * - Lock-off ESD Urethane Casters (adds 1" to seat height) [ELOF] |

