airCentric™Boardroom [air-BR]

|  |  |
| --- | --- |
| Backrest* 5" Patented Back Height Adjustment System
* Front Upholstered Dual Curve Backrest (19"w x 24"h)
* Plastic Back Cap with Airflow Vents
* Proprietary Airflow Molded Polyurethane Foam and Structure

Arms* [Click here](http://ergocentric.com/resource/arms) to view options

Seat* Tailored Upholstery on Seat Pan (20”w x 19”d)
* Proprietary Airflow Molded Polyurethane Foam and Structure

**Options:*** Extra Long Non-Airflow Seat (20”w x 21”d) [XLS]
* Small Non-Airflow Seat (18.5”w x 17”d) [SS]
* Triple Density Foam (adds ¼” to seat width and depth) (Not available on airCentric seat options) [TDF]
* Standard Non-Airflow Seat (20”w x 19”d) [LS]
* airCentric Plus Size Seat (22”w x 19”d) [ACPS]]
* airCentric Small Seat (18.5”w x 17”d) [ACSS]

Boardroom Mechanism* Adjustable Spring Tension
* Seat Height
* Single Tilt Lock Free Float

Pneumatic Lift (Seat Height)* 125 mm Pneumatic Lift (16" - 21")

**Options:*** 80 mm Pneumatic Lift (only available with 26” Glass Reinforced Nylon Base) (15”-18”) [80mm]
* 100 mm Pneumatic Lift (15.5”-19”) [100mm]
* 140 mm Pneumatic Lift (17”-22.5”) [140mm]
* Memory Gas Column (17”) [MGC]
 | Base/Glides/Casters* 25" Glass Reinforced Nylon High Profile Base
* 5 Dual Wheel Nylon Carpet Casters

**Options:*** Chrome Accent Casters [CAC]
* 26” Polished Aluminum Base [PB]
* Urethane Casters [UC]
* 26” Glass Reinforced Nylon Base [26NB]
 |