geoCentric Counter Stool [geo-STOOL]

|  |  |
| --- | --- |
| Backrest   * Backrest 18.25" wide by 12.5" high * Concealed Back Brackets (except when upholstered in vinyl or leather) * Dual Curve Backrest   Seat   * 31.25" Seat Height * Dual Curve Waterfall Seat * Seat Pan 18.5" wide by 19.5" deep | Base/Glides/Casters  **Options:**   * Metal Sled base option with glass reinforced nylon glides (SLED)   Frame   * 14 Gauge, 7/8" Steel Tube Frame * Black Textured Semi-Gloss Powder Coat Paint * Kick Back Legs for Stability with Durable Custom Glides * Step 12" high   **Options**   * Counter stool chrome frame (CCF)   Additional Options   * Cal. 133 [Cal133] * Ganging clips (set of 2) chair with no arms [GCNA] |