geoCentric Stacker Armless [geo-STACKER]

|  |  |
| --- | --- |
| Backrest* Backrest 18.25" wide by 12.5" high
* Concealed Back Brackets (except when upholstered in vinyl or leather)
* Dual Curve Backrest

Seat* 17" Seat Height
* Dual Curve Waterfall Seat
* Seat Pan 18.5" wide by 19.5" deep
 | Base/Glides/Casters**Options:*** Nylon Stacker Casters [NSC]
* Urethane Stacker Casters [USC]
* Metal Sled base option with glass reinforced nylon glides (chair does not stack with sled base option) [SLED]

Frame* 14 Gauge, 7/8" Steel Tube Frame
* Black Textured Semi-Gloss Powder Coat Paint
* Kick Back Legs for Stability with Durable Custom Glides

**Options*** Chrome frame (CF)
* Wall saver frame (SWS)

Additional Options* Cal. 133 [Cal133]
* Cart (23" wide by 29.75" long by 14.75" high) Stackable 6 units high without cart and 10 units high with cart [CART]
* Ganging clips (set of 2) chair with arms [GC]

Measurements / Overall DimensionsBoxed Weight/Size (21 lbs./13 cu.ft) |