ecoCentric™ MeshBoardroom [eco-MESH-BR]

|  |  |
| --- | --- |
| Backrest   * Mesh backrest 19.25”w x 23”h * 4” of adjustable lumbar support   Arms   * [Click here](http://ergocentric.com/resource/arms) to view options   Seat   * Eight Ply Hardwood Seat Structure * High Resilient Polyurethane Foam * Tailored Upholstery on seat Pan (20”w x19”d)   **Options:**   * Extra Long Seat (20”w x 21”d) [XLS] * Large Airflow Seat (20”w x 19”d) [LSAF] * Small Airflow Seat (18.5”w x 17”d) [SSAF] * Small Seat (18.5”w x 17”d) [SS] * Triple Density Foam Seat (Adds ¼” to seat width and depth) [TDF]   Boardroom Mechanism   * Seat Height * Single Lock Free Float * Adjustable Spring Tension   Pneumatic Lift (Seat Height)   * 125 mm Pneumatic Lift (16" - 21")   **Options:**   * 80 mm Pneumatic Lift (only available with 26” Glass Reinforced Nylon Base)[26NB] (15”-18”) [80mm] * 100 mm Pneumatic Lift (15.5”-19”) [100mm] * 140 mm Pneumatic Lift (17.25”-22.75”) [140mm] * Memory Gas Column (17”) [MGC] | Base/Glides/Casters   * 25" Glass Reinforced Nylon High Profile Base * 5 Dual Wheel Nylon Carpet Casters   **Options:**   * 26” Glass Reinforced Nylon Base [26NB] * Chrome Accent Casters [CAC] * 26” Polished Aluminum Base [PB] * Single Wheel Casters [SW] * Single Wheel Urethane Casters [SWU] * Urethane Casters [UC] * 2 ¼” Glides [2G]   Additional Options   * Adjustable Headrest [AHR] * Cal. 133 [Cal133] |