ecoCentric™ MeshBoardroom [eco-MESH-BR]

|  |  |
| --- | --- |
| Backrest* Mesh backrest 19.25”w x 23”h
* 4” of adjustable lumbar support

Arms* [Click here](http://ergocentric.com/resource/arms) to view options

Seat* Eight Ply Hardwood Seat Structure
* High Resilient Polyurethane Foam
* Tailored Upholstery on seat Pan (20”w x19”d)

**Options:*** Extra Long Seat (20”w x 21”d) [XLS]
* Large Airflow Seat (20”w x 19”d) [LSAF]
* Small Airflow Seat (18.5”w x 17”d) [SSAF]
* Small Seat (18.5”w x 17”d) [SS]
* Triple Density Foam Seat (Adds ¼” to seat width and depth) [TDF]

Boardroom Mechanism* Seat Height
* Single Lock Free Float
* Adjustable Spring Tension

Pneumatic Lift (Seat Height)* 125 mm Pneumatic Lift (16" - 21")

**Options:*** 80 mm Pneumatic Lift (only available with 26” Glass Reinforced Nylon Base)[26NB] (15”-18”) [80mm]
* 100 mm Pneumatic Lift (15.5”-19”) [100mm]
* 140 mm Pneumatic Lift (17.25”-22.75”) [140mm]
* Memory Gas Column (17”) [MGC]
 | Base/Glides/Casters* 25" Glass Reinforced Nylon High Profile Base
* 5 Dual Wheel Nylon Carpet Casters

**Options:*** 26” Glass Reinforced Nylon Base [26NB]
* Chrome Accent Casters [CAC]
* 26” Polished Aluminum Base [PB]
* Single Wheel Casters [SW]
* Single Wheel Urethane Casters [SWU]
* Urethane Casters [UC]
* 2 ¼” Glides [2G]

Additional Options* Adjustable Headrest [AHR]
* Cal. 133 [Cal133]

  |