ecoCentric™ StudentSeat Height [eco-STUDENT]

|  |  |
| --- | --- |
| Backrest   * Dual Curve Plastic Back (20”w x 12.5”h) * Handle in back for easy movement * Unique Scalloped Indentations for the spine   Back and Seat Frame   * 14 Gauge, 7/8” Steel Tube Frame * Black Textured Semi-Gloss Powder Coat Paint   Seat   * 18”w x 18.5”d * Dual Curve Waterfall Plastic Seat in Black * Unique Scalloped Indentations for the Seat Bones   **Options:**   * Grey Package (Includes Grey Seat and Backrest) * Upholstered Seat [UPHS]   Seat Height Mechanism   * Seat Height   Pneumatic Lift (Seat Height)   * 125 mm Pneumatic Lift (14.5" – 19.5")   **Options:**   * 80 mm Pneumatic Lift (13.5”-16.5”) [80mm] * 100 mm Pneumatic Lift (14”-17.5”) [100mm] * 140 mm Pneumatic Lift (15.25”-20.75”) [140mm] * 157 mm Pneumatic Lift (17.25”-23”) [157mm] * 200 mm Pneumatic Lift (Includes upgrade to 26” base for stability) (20.5”-27.5”) [200mm] * 267 mm Pneumatic Lift (23”-33”) [267mm] | Base/Glides/Casters   * 24” Glass Reinforced Nylon Base * 5 Dual Wheel Nylon Carpet Casters   **Options:**   * 2 ¼” Glides [2G] * 20” Diameter Height Adjustable Footring (for use as a foot rest only) [20FR] * Single Wheel Casters [SW] * Single Wheel Urethane Casters [SWU] * Urethane Casters [UC] * 26” Glass Reinforced Nylon Base [26NB]   Additional Options   * Grey Plastic Backrest (20”w x 12.5”h) [PLABG] * Grey Plastic Seat (18”w x 18.5”d) [PLASG] |