ergoForce High BackPlus Size Multi Tilt [eForce-HB-PLUS-350MT]

|  |  |
| --- | --- |
| Backrest   * 5" Patented Back Height Adjustment System * Abrasion resistant strip on bottom of backrest 7” high * Fully Upholstered Dual Curved Backrest (19”w x 26”h) * Heavy Duty Back Bar Support * Molded Polyurethane Foam   Arms   * [Click here](http://ergocentric.com/resource/arms) to view options   Seat   * Abrasion resistant strip on back of seat * Eight Ply Hardwood Seat Structure * High Resilient Polyurethane Foam * Seat Pan 22" wide by 19" deep   **Options:**   * Extra Large Seat (22"Wx21"D) [SS] * Triple Density Foam Seat (Adds 1/4" to seat width and depth) [TDF] * Tailored Upholstery on Seat Pan [TS]   Heavy Duty Multi Tilt Mechanism   * Forward Tilt Lock Out * Adjustable Spring Tension * Infinite Lock Free Float * 2.5" Depth Adjustable Seat Slider * Back Angle Adjustment   Pneumatic Lift (Seat Height)   * 125 mm Pneumatic Lift Heavy Duty   (seat height -17.5"-22.5")  **Options:**   * 80 mm Heavy Duty pneumatic lift (17"-20") [80mm] * 100 mm Heavy Duty pneumatic lift (17.25-20.75") [100mm] * 140 mm Heavy Duty pneumatic lift (18"-23.5") [140mm] | Base/Glides/Casters   * 27" Hercules Glass Reinforced Nylon Base * 5 Dual Wheel Nylon Carpet Casters   **Options:**   * 2 1/4" Glides [2G] * Chrome Accent Casters [CAC] * Single Wheel Casters [SW] * Single Wheel Urethane Casters [SWU] * Urethane Casters [UC]   Additional Options   * Air Lumbar [AL] * Air Thoracic [AT] * Air Thoracic and Air Lumbar [ATL] * Adjustable Headrest [AHR] * Heavy Duty Control (Task Intensive) [TI] |