tCentric Hybrid™

|  |  |
| --- | --- |
| All Mesh - Synchro Glide\* | Midnight Black [t-MBMESH-SG] |
| Light Grey [t-LGMESH-SGG] |
| Backrest:   * 5" Patented Back Height Adjustment System * Dual Curve Mesh Backrest (19"w x 25"h)   Arms:  Midnight Black / Light Grey [G]   * TC Armrest Height & Lateral [TCL / TCLG] * TC Armrest Height & Swivel [TC360 / TC360G] * TC Armrest Height, Lateral & Swivel [TCL360 / TCL360G]   Seat: Midnight Black / Light Grey   * Airless Cushion Technology * Mesh Seat with 30% Glass Filled Nylon Frame (21”w x 18 ½”d)   **Options:**  *Midnight Black [MB] / Light Grey [G]*   * Small Mesh Seat (20”w x 16 ½”d) [TMBMSS / TLGMSS] * Extra Long Mesh Seat (21”w x 20 ½”d) [TMBMXLS / TLGMXLS]   Pneumatic Lift (Seat Height): Midnight Black / Light Grey   * 125 mmLT Pneumatic Lift (18 ¾" – 23 ½")   Synchro Glide Mechanism:  Midnight Black / Light Grey   * 1 ¾” Depth Adjustable Seat Slider * Adjustable Spring Tension * Free Float * Independent Back Angle Adjustment * Seat Tilt Lock Out * Synchro 2:1 Ratio   **Options:**  *Midnight Black / Light Grey [G]*   * 70 mm Pneumatic Lift (18 ¼” – 21”) [70MM/G70MM] * 80 mm Pneumatic Lift (19”-22”) [80MM/G80MM] * 100 mm Pneumatic Lift (19 ½”-23 ¼”) [100MM/G100MM] * 140 mm Pneumatic Lift (20 ¾”-26 ¼”) [140MM/G140MM]   *Chrome*   * 100 mm Chrome Pneumatic Lift (19 ½”-23 ¼”) [100MMCH] * 125 mm Chrome Pneumatic Lift (19 ¾”-24 ½”) [125MMCH] * 140 mm Chrome Pneumatic Lift (20 ¾”-26 ¼”) [140MMCH] | Base/Glides/Casters:  Midnight Black / Light Grey   * 26" Glass Reinforced Nylon Mid-Profile Base * 5 Dual Wheel Nylon Casters 2   **Options:**   * Chrome Accent Casters [CAC] * 26” Polished Aluminum Mid-Profile Base [PMB] * Dual Wheel Urethane Caster 2 [UC2]   Additional Options:  Midnight Black / Light Grey [G]   * tCentric Lumbar Support [TLS / TLSG] * tCentric Lumbar Support with Air Lumbar (pump) [TLSAL / TLSALG] * Adjustable Headrest [AHR / AHRG]   Measurements/Overall Dimensions:   * Boxed Weight/Size: 46.4 lbs./11.7 cu.ft.   Mesh Material:  Both the tCentric Hybrid seat and backrest are made from elastomeric mesh with fill yarns made from polyester.  When stretched, this material yields excellent load-bearing properties and resiliency, showing less than 5% load-bearing loss when tested according to BIFMA standards.  To clean use mild household or hospital detergents.  \*Mixing of Midnight Black & Light Grey components is not an option. |

­