eCentric High BackKnee Tilt [e-HB-KT]

|  |  |
| --- | --- |
| Backrest   * 20" wide by 27" high * 5" Patented Back Height Adjustment System * Fully Upholstered Dual Curved Backrest * Molded Polyurethane Foam   Arms   * [Click here](http://ergocentric.com/resource/arms) to view options   Seat   * Eight Ply Hardwood Seat Structure * High Resilient Polyurethane Foam * Seat Pan 20" wide by 19" deep   **Options:**   * Memory Foam Seat [EA] * Extra Long Seat (20"Wx21"D) [XLS] * Small Seat (18.5"Wx17"D) [SS] * Triple Density Foam Seat (Adds 1/4" to seat width and depth) [TDF] * Tailored Upholstery on Seat Pan [TS]   Knee Tilt Mechanism   * Adjustable Spring Tension * Infinite Lock Free Float * 2.5" Depth Adjustable Seat Slider * Back Angle Adjustment   Pneumatic Lift (Seat Height)   * 125 mm Pneumatic Lift (seat height -17.5"-22.5")   **Options:**   * 80 mm pneumatic lift (17"-20") [80mm] * 100 mm pneumatic lift (17.25-20.75") [100mm] * 140 mm pneumatic lift (18"-23.5") [140mm] | Base/Glides/Casters   * 27" Hercules Glass Reinforced Nylon Base * 5 Dual Wheel Nylon Carpet Casters   **Options:**   * 2 1/4" Glides [2G] * Chrome Accent Casters [CAC] * 26" Polished Aluminum Base [PB] * Single Wheel Casters [SW] * Single Wheel Urethane Casters [SWU] * Urethane Casters [UC]   Additional Options   * Air Lumbar (AL) * Thoracic Back Support [THB] * Adjustable Headrest [AHR] * Cal. 133 [Cal133] |