tCentric Hybrid™ Synchro Glide [t-SG]

|  |  |
| --- | --- |
| Backrest   * 5" Patented Back Height Adjustment System * Dual Curve Mesh Backrest (19"w x 25"h)   Arms   * TC Armrest Height & Lateral [TCL] * TC Armrest Height & Swivel [TC360] * TC Armrest Height, Lateral & Swivel [TCL360]   Seat   * Mesh Seat with 30% Glass Filled Nylon Frame * Airless Cushion Technology * Seat Pan 21"w x 19"d   **Six upholstered seat sizes options:**   * Extra Small (17.5w" x 15.5"d) [XSS] * Small (18.5"w x 17"d) [AFSS] * Standard (20"w x 19"d) [LS] * Plus Size (22"w x 19"d) [PS] * Extra Long Seat (20"w x 21"d) [XLS] * Extra Deep (22"w x 21"d) [XPS]   Synchro Glide Mechanism   * 2.5" Depth Adjustable Seat Slider * Adjustable Spring Tension * Free Float * Independent Back Angle Adjustment * Seat Tilt Lock Out * Synchro 2:1 Ratio   Pneumatic Lift (Seat Height)   * 125 mm Pneumatic Lift (18"-23")   **Options:**   * 100 mm Pneumatic Lift (17.5"-21") *100mm* * 140 mm Pneumatic Lift (19"-24.5") *140mm* * 80 mm Pneumatic Lift (17.25"-20.25") *80mm* * 100 mm Pneumatic Lift Chrome (17.5"-21") *100mmCH* * 125 mm Pneumatic Lift Chrome (18"-23") *25mmCH* * 140 mm Pneumatic Lift Chrome (19"-24.5") *140mmCH* | Base/Glides/Casters   * 26" Glass Reinforced Nylon High Profile Base 2 * 5 Dual Wheel Nylon Carpet Casters 2   **Options:**   * Chrome Accent Casters [CAC] * 26" Polished Aluminum High Profile Base [PB2] * Urethane Caster [UC2]   Additional Options   * Adjustable Headrest [AHR] * CooltoTouch Lumbar Support (12"w x 6"h) [TLS] * CooltoTouch Lumbar Support with Air Lumbar [TLSAL]   Measurements/Overall Dimensions  Boxed Weight (60.65 lbs.)    Mesh Material  Both the tCentric Hybrid seat  and backrest are made from  elastomeric mesh with fill  yarns made from polyester.  When stretched, this material  yields excellent load-bearing  properties and resiliency,  showing less than 5% load-bearing loss when tested according to BIFMA standards.  To clean use mild household or hospital detergents. |