ergoCentric3-in-1 Sit Stand [3 in 1 Sit Stand]

|  |  |  |  |
| --- | --- | --- | --- |
| Backrest   * Fully upholstered backrest (14"w x 10"h) * 4" of back height adjustment   Seat   * Upholstered seat with dual density molded polyurethane Foam with 5" ergoCentric+Guard™ No-Slip Strip * Seat pan 17.5" wide by 15.5" deep  |  |  | | --- | --- | |  | *Options*:  > 3-in-1 Large seat pan (18.5"w x 17"d) [SS] |   Dedicated Task Control 2   * 1 Lever for both seat and back angle adjustment * Back height adjustment * Back pivot * Seat height   Pneumatic Lift (Seat Height)   * 200mm Knurled dual height adjustment system  (seat height 7.5" of adjustment between 19.25"- 35.5")   Base/Glides/Casters   * 22" Chrome 22 base has an 18" oval tube foot ring  built in for durability * 2 x 2 ¼" Dual wheel nylon casters and 3 x 2 ¼" glides * Options: * 5 x 2 ¼" Glides [2G] * 2 x Urethane casters and 2 x 2 ¼" glides [2UC32G]   Additional Options   * 3-in-1 High Back (17"w x 15"h) [3N1HB] * Cal. 133 [Cal133] |  |