ergoForce Mid Back24 Hour Multi Tilt [eForce-MB-24MT]

|  |  |
| --- | --- |
| Backrest* 15.5" wide by 19" high
* 5" Patented Back Height Adjustment System
* Abrasion resistant ergoCentric+Guard strip on bottom of backrest
* Heavy Duty Back Bar Support
* Fully Upholstered Dual Curved Backrest
* Molded Polyurethane Foam

 Arms* [Click here](http://ergocentric.com/resource/arms) to view options

Seat* Abrasion resistant ergoCentric+Guard strip on back of seat
* Eight Ply Hardwood Seat Structure
* High Resilient Polyurethane Foam
* Seat Pan 20" wide by 19" deep

**Options:*** Memory Foam Seat [EA]
* Extra Long Seat (20"Wx21"D) [XLS]
* Small Seat (18.5"Wx17"D) [SS]
* Triple Density Foam Seat (Adds 1/4" to seat width and depth) [TDF]
* Tailored Upholstery on Seat Pan [TS]

24 Hour Multi Tilt Mechanism* Back Angle Adjustment
* Adjustable Spring Tension
* Forward Tilt Lock Out
* Infinite Lock Free Float
* 2.5" Depth Adjustable Seat Slider

 Pneumatic Lift (Seat Height)* 125 mm Pneumatic Lift (seat height -17.5"-22.5")

**Options:*** 80 mm pneumatic lift (17"-20") [80mm]
* 100 mm pneumatic lift (17.25-20.75") [100mm]
* 140 mm pneumatic lift (18"-23.5") [140mm]
 | Base/Glides/Casters* 26” Glass Reinforced Nylon Base
* 5 Dual Wheel Nylon Carpet Casters

 **Options:*** 2 1/4" Glides [2G]
* Chrome Accent Casters [CAC]
* Single Wheel Casters [SW]
* Single Wheel Urethane Casters [SWU]
* Urethane Casters [UC]

Additional Options* Air Lumbar [AL]
* Air Thoracic [AT]
* Air Thoracic and Air Lumbar [ATL]
* Adjustable Headrest [AHR]
* Heavy Duty Control (Task Intensive) [TI]

Measurements / Overall Dimensions* Boxed Weight/Size 72 lbs/11.7 cu.ft
 |