tCentric Hybrid™Counter Height [t-CH]

|  |  |
| --- | --- |
| Backrest   * 5" Patented Back Height Adjustment System Dual Curve Mesh Backrest (19"w x 25"h)   Arms   * [Click here](http://ergocentric.com/resource/arms) to view options   Seat   * Eight Ply Hardwood Seat Structure * Seat Pan 20" wide by 19" deep * Dual Density Molded Polyurethane   **Options:**   * Memory Foam Seat [EA] * Extra Long Seat (20"w x 21"d) [XLS] * Small Seat (18.5"wx17"d) [SS] * Triple Density Foam Seat (Adds 1/4" to seat width and depth) [TDF]   Dedicated Task Mechanism   * Independent Back Angle Adjustment * Seat Angle Adjustment * Seat Height   Pneumatic Lift (Seat Height)   * 200 mm Pneumatic Lift (20.5" - 27.5")   **Options:**   * 157 mm Pneumatic Lift (16.25”-22.25”) [157mm] * 267 mm Pneumatic Lift (23”-33”) [267mm] | Base/Glides/Casters   * 20” Diameter Height Adjustable Footring * 26” Glass Reinforced Nylon Base * 1 ¼” Glides   **Options:**   * 2 ¼” Glides [2G] * Nylon Casters [NC] * Lock Off Urethane Casters [LOF] * Lock On Urethane Casters [LON] * Single Wheel Casters [SW] * Single Wheel Urethane Casters [SWU] * Urethane Casters [UC]   Additional Options   * Adjustable Headrest [AHR] * CooltoTouch Lumbar Support (12"w x 6"h) [TLS] * CooltoTouch Lumbar Support with Air Lumbar [TLSAL]   Measurements / Overall Dimensions  Boxed Weight/Size (56 lbs./6.7 cu.ft) |