tCentric Hybrid™Counter Height [t-CH]

|  |  |
| --- | --- |
| Backrest* 5" Patented Back Height Adjustment SystemDual Curve Mesh Backrest (19"w x 25"h)

Arms* [Click here](http://ergocentric.com/resource/arms) to view options

Seat* Eight Ply Hardwood Seat Structure
* Seat Pan 20" wide by 19" deep
* Dual Density Molded Polyurethane

**Options:*** Memory Foam Seat [EA]
* Extra Long Seat (20"w x 21"d) [XLS]
* Small Seat (18.5"wx17"d) [SS]
* Triple Density Foam Seat (Adds 1/4"to seat width and depth) [TDF]

Dedicated Task Mechanism* Independent Back Angle Adjustment
* Seat Angle Adjustment
* Seat Height

Pneumatic Lift (Seat Height)* 200 mm Pneumatic Lift (20.5" - 27.5")

**Options:*** 157 mm Pneumatic Lift (16.25”-22.25”) [157mm]
* 267 mm Pneumatic Lift (23”-33”) [267mm]
 | Base/Glides/Casters* 20” Diameter Height Adjustable Footring
* 26” Glass Reinforced Nylon Base
* 1 ¼” Glides

**Options:*** 2 ¼” Glides [2G]
* Nylon Casters [NC]
* Lock Off Urethane Casters [LOF]
* Lock On Urethane Casters [LON]
* Single Wheel Casters [SW]
* Single Wheel Urethane Casters [SWU]
* Urethane Casters [UC]

Additional Options* Adjustable Headrest [AHR]
* CooltoTouch Lumbar Support (12"w x 6"h) [TLS]
* CooltoTouch Lumbar Support with Air Lumbar [TLSAL]

Measurements / Overall DimensionsBoxed Weight/Size (56 lbs./6.7 cu.ft) |