airCentric™Synchro Glide [air-SG]

|  |  |
| --- | --- |
| Backrest   * 5" Patented Back Height Adjustment System * Front Upholstered Dual Curve Backrest (19"w x 24"h) * Plastic Back Cap with Airflow Vents * Proprietary Airflow Molded Polyurethane Foam and Structure   Arms   * [Click here](http://ergocentric.com/resource/arms) to view options   Seat   * Tailored Upholstery on Seat Pan (20”w x 19”d) * Proprietary Airflow Molded Polyurethane Foam and Structure   **Options:**   * Extra Long Non-Airflow Seat (20”w x 21”d) [XLS] * Small Non-Airflow Seat (18.5”w x 17”d) [SS] * Triple Density Foam (adds ¼” to seat width and depth) (Not available on airCentric seat options) [TDF] * Standard Non-Airflow Seat (20”w x 19”d) [LS] * airCentric Plus Size Seat (22”w x 19”d) [ACPS]] * airCentric Small Seat (18.5”w x 17”d) [ACSS]   Synchro Glide Mechanism   * 2.5” Depth Adjustable Seat Slider * Adjustable Spring Tension * Free Float * Independent Back Angle Adjustment * Seat Tilt Lock Out * Synchro 2:1 Ratio   Pneumatic Lift (Seat Height)   * 125 mm Pneumatic Lift (18" – 23")   **Options:**   * 80 mm Pneumatic Lift (only available with 26” Glass Reinforced Nylon Base) (17.25”-20.25”) [80mm] * 100 mm Pneumatic Lift (17.5”-21”) [100mm] * 140 mm Pneumatic Lift (19”-24.5”) [140mm] | Base/Glides/Casters   * 25" Glass Reinforced Nylon High Profile Base * 5 Dual Wheel Nylon Carpet Casters   **Options:**   * 2 ¼” Glides [2G] * Chrome Accent Casters [CAC] * 26” Polished Aluminum Base [PB] * Single Wheel Casters [SW] * Single Wheel Urethane Casters [SWU] * Urethane Casters [UC] * 26” Glass Reinforced Nylon Base [26NB]   Additional Options   * Air Lumbar [AL] * Memory Foam Seat (Not Available on airCentric seat options) [EA] * Adjustable Headrest [AHR] * Cal. 133 [Cal133] |