airCentric™Synchro [air-S]

|  |  |
| --- | --- |
| Backrest* 5" Patented Back Height Adjustment System
* Front Upholstered Dual Curve Backrest (19"w x 24"h)
* Plastic Back Cap with Airflow Vents
* Proprietary Airflow Molded Polyurethane Foam and Structure

Arms* [Click here](http://ergocentric.com/resource/arms) to view options

Seat* Tailored Upholstery on Seat Pan (20”w x 19”d)
* Proprietary Airflow Molded Polyurethane Foam and Structure

**Options:*** Extra Long Non-Airflow Seat (20”w x 21”d) [XLS]
* Small Non-Airflow Seat [SS]
* Triple Density Foam (adds ¼” to seat width and depth) (Not available on airCentric seat options) [TDF]
* Standard Non-Airflow Seat (20”w x 19”d) [LS]
* airCentric Plus Size Seat (22”w x 19”d) [ACPS]]
* airCentric Small Seat (18.5”w x 17”d) [ACSS]

Synchro Mechanism* 2.5” Depth Adjustable Seat Slider
* Adjustable Spring Tension
* Infinite Lock Free Float
* Synchro 2:1 Ratio

Pneumatic Lift (Seat Height)* 125 mm Pneumatic Lift (16" - 21")

**Options:*** 80 mm Pneumatic Lift (only available with 26” Glass Reinforced Nylon Base) (15.25”-18.25”) [80mm]
* 100 mm Pneumatic Lift (15.5”-19”) [100mm]
* 140 mm Pneumatic Lift (17”-22.5”) [140mm]
 | Base/Glides/Casters* 25" Glass Reinforced Nylon High Profile Base
* 5 Dual Wheel Nylon Carpet Casters

**Options:*** 2 ¼” Glides [2G]
* Chrome Accent Casters [CAC]
* 26” Polished Aluminum Base [PB]
* Single Wheel Casters [SW]
* Single Wheel Urethane Casters [SWU]
* Urethane Casters [UC]
* 26” Glass Reinforced Nylon Base [26NB]

Additional Options* Air Lumbar [AL]
* Memory Foam Seat (Not Available on airCentric seat options) [EA]
* Adjustable Headrest [AHR]
* Cal. 133 [Cal133]

  |