ecoCentric II Mid BackBoardroom [eco-MB-ACCENT-II]

|  |  |
| --- | --- |
| Backrest* Backrest (Single Pull Through) (17”w x 18.5”h)

 Arms* Eco II Arms

Seat* Seat Pan (Single Pull Through) (20.5”w x 18.5”d)

Accent Mechanism* Infinite Lock Free Float
* Seat Height
* Adjustable Spring Tension

**Options:*** 2-Position Lock Swivel Tilt Mechanism (lowers seat height by 0.5”) [2ST]

 Pneumatic Lift (Seat Height)* 125 mm Pneumatic Lift (seat height -19"-24")

**Options:*** 80 mm pneumatic lift (18-20.21") [80mm]
* 100 mm pneumatic lift (18.25-21.75") [100mm]
* 140 mm pneumatic lift (20-25.5") [140mm]
* Memory Gas Column (20”) [MGC]
 | Base/Glides/Casters* 25" Glass Reinforced Nylon High Profile Base
* 5 Dual Wheel Nylon Carpet Casters

 **Options:*** 2 1/4" Glides [2G]
* 26” Glass Reinforced Nylon Base [26NB]
* Jury base (with cover) [JURY1]
* Jury base (without cover) [JURY2]
* Chrome Accent Casters [CAC]
* 26" Polished Aluminum Base [PB]
* Single Wheel Casters [SW]
* Single Wheel Urethane Casters [SWU]
* Urethane Casters [UC]

Frame* Single Shell Structure

Additional Options* Executive Boardroom Mechanism [EXBR]
* Nytek Arm Cover [NY]
* Pleated Back [PLB]
* Pleated Seat [PLS]
* Adjustable Headrest [AHR]

  |