ecoCentric™ MeshMulti Tilt [eco-MESH-MT2]

|  |  |
| --- | --- |
| Backrest* Mesh backrest (19.25”w x 23”h)
* 4” of adjustable lumbar support

Arms* [Click here](http://ergocentric.com/resource/arms) to view options

Seat* Eight Ply Hardwood Seat Structure
* High Resilient Polyurethane Foam
* Tailored Upholstery on Seat Pan 20”w x 19”d

**Options:*** Memory Foam Seat [EA]
* Extra Long Seat (20”w x 21”d) [XLS]
* Large Airflow Seat (20”w x 19”d) [LSAF]
* Small Airflow Seat (18.5”w x 17”d) [SSAF]
* Small Seat (18.5”w x 17”d) [SS]
* Triple Density Foam Seat (Adds ¼” to seat width and depth) [TDF]

Multi Tilt Mechanism* 2.5” Depth Adjustable Seat Slider
* Adjustable Spring Tension
* Back Angle Adjustment
* Infinite Forward Tilt Lock Out
* Infinite Lock Free Float

Pneumatic Lift (Seat Height)* 125 mm Pneumatic Lift (16.5" – 21.5")

**Options:*** 80 mm Pneumatic Lift (only available with 26” base [26NB] (15.75”-18.75”) [80mm]
* 100 mm Pneumatic Lift (16”-19.5”) [100mm]
* 140 mm Pneumatic Lift (17.5”-23”) [140mm]
 | Base/Glides/Casters* 25” Glass Reinforced Nylon High Profile Base
* 5 Dual Wheel Nylon Carpet Casters

**Options:*** 26” Glass Reinforced Nylon Base [26NB]
* Chrome Accent Casters [CAC]
* 26” Polished Aluminum Base [PB]
* Single Wheel Casters [SW]
* Single Wheel Urethane Casters [SWU]
* Urethane Casters [UC]
* 2 ¼” Glides [2G]

Additional Options* 24 Hour Multi Tilt Mechanism (Warranted for 24 hour use up to a weight of 280 lbs.) [24MT]
* Adjustable Headrest [AHR]
* Cal. 133 [Cal133]

  |