ergoCentricBariatric Task Chair [BART]

|  |  |
| --- | --- |
| Backrest* Customized upholstered backrest
* Uses 2 heavy duty back bar supports
* Height range \* (22” – 28” high)
* Width range \* (20” – 28” wide)

Arms* Available fixed arm heights from seat pan: 7", 8", 9", 10"
* Oval black destiny upholstered padded arm pad 6 ½" wide by 11 ¾" long
* Solid 3" wide by ¼" thick high tensile steel bar powder coated black
* Steel arm brackets are welded to mechanisms to avoid excess weight to seat pan
* Arm width adjustable of 2" per arm
* [Click here](http://ergocentric.com/resource/arms) to view options

Seat* Customized upholstered seat pan
* 16" to 24" depth range
* 24" to 34" width range

BT Control* 2 Heavy Duty Task Mechanisms' adjustment controls work in tandem
* Back angle
* Seat height
* Seat tilt
* Side tension

Pneumatic Lift (Seat Height)* High Pressure, high capacity cylinder
* Seat Height (18” – 22.25”)
 | Base/Glides/Casters* 30” Diameter Steel Base
* 6 Dual wheel, heavy duty casters are industrial grade

Additional Options* Cal. 133 [Cal133]

 |