ergoCentricBariatric Task Chair [BART]

|  |  |
| --- | --- |
| Backrest   * Customized upholstered backrest * Uses 2 heavy duty back bar supports * Height range \* (22” – 28” high) * Width range \* (20” – 28” wide)   Arms   * Available fixed arm heights from seat pan: 7", 8", 9", 10" * Oval black destiny upholstered padded arm pad 6 ½" wide by 11 ¾" long * Solid 3" wide by ¼" thick high tensile steel bar powder coated black * Steel arm brackets are welded to mechanisms to avoid excess weight to seat pan * Arm width adjustable of 2" per arm * [Click here](http://ergocentric.com/resource/arms) to view options   Seat   * Customized upholstered seat pan * 16" to 24" depth range * 24" to 34" width range   BT Control   * 2 Heavy Duty Task Mechanisms' adjustment controls work in tandem * Back angle * Seat height * Seat tilt * Side tension   Pneumatic Lift (Seat Height)   * High Pressure, high capacity cylinder * Seat Height (18” – 22.25”) | Base/Glides/Casters   * 30” Diameter Steel Base * 6 Dual wheel, heavy duty casters are industrial grade   Additional Options   * Cal. 133 [Cal133] |