geoCentric Extra High BackSynchro [geo-XHB-S]

|  |  |
| --- | --- |
| Backrest* Fully Upholstered Dual Curve Backrest
* 19" wide by 34" high
* 5" Patented Back Height Adjustment System

Arms* [Click here](http://ergocentric.com/resource/arms) to view options

Seat* Eight Ply Hardwood Seat Structure
* High Resilient Polyurethane Foam
* Seat Pan 20" wide by 19" deep

**Options:*** Memory Foam Seat [EA]
* Small Seat (18.5"W x 17"D) [SS]
* Extra Long Seat (20"Wx21"D) [XLS]
* Triple Density Foam Seat (Adds 1/4" to seat width and depth) [TDF]
* Tailored Upholstery on Seat Pan [TS]

Synchro Mechanism * 2.5" Depth Adjustable Seat Slider
* Adjustable Spring Tension
* Infinite Lock Free Float
* Synchro 2:1 Ratio

Pneumatic Lift (Seat Height)* 125 mm Pneumatic Lift (16" – 21")

**Options:*** 80 mm pneumatic lift (15.25-18.25") [80mm]
* 100 mm pneumatic lift (15.5-19") [100mm]
* 140 mm pneumatic lift (17-22.5") [140mm]
 | Base/Glides/Casters* 26" Glass Reinforced Nylon Base
* 5 Dual Wheel Nylon Carpet Casters

**Options:*** 2 1/4" Glides [2G]
* Chrome Accent Casters [CAC]
* 26" Polished Aluminum Base [PB]
* Single Wheel Nylon Casters [SW]
* Single Wheel Urethane Casters [SWU]
* Urethane Casters [UC]

Additional Options* Air Lumbar [AL]
* Air Thoracic [AT]
* Air Thoracic and Air Lumbar [ATL]
* Cal. 133 [Cal133]
* Neck Support [NNS]

Measurements / Overall DimensionsBoxed Weight/Size (60 lbs./11.7 cu.ft)  |