airCentric™2

|  |  |  |
| --- | --- | --- |
| Knee Tilt | Midnight Black [air2-KT] | |
|  | | |
| Backrest   * 5" Patented Back Height Adjustment System * Front Upholstered Dual Curve Backrest (19"w x 24"h) * Plastic Back Cap with Airflow Vents * Proprietary Airflow Molded Polyurethane Foam and Structure   Arms   * [Click here](http://ergocentric.com/resource/arms) to view options   Seat   * Tailored Upholstery on Seat Pan (20”w x 19”d) * Proprietary Airflow Molded Polyurethane Foam and Structure   **Options:**   * Extra Small (17.5”w x 15.5d) [XSS] * Small Seat (18.5”w x 17”d) [SS] * Plus Size (18.”w x 19”d) [PS] * Extra Long Seat (20”w x 21”d) [XLS] * Standard Seat (20”w x 19”d) [LS] * Triple Density Foam (adds ¼” to seat width and depth) [TDF]   Pneumatic Lift (Seat Height)   * 125 mm Pneumatic Lift (18" – 23")   **Options:**   * 80 mm Pneumatic Lift (only available with 26” Glass Reinforced Nylon Base) (17.25”-20.25”) [80mm] * 100 mm Pneumatic Lift (17.5”-21”) [100mm] * 140 mm Pneumatic Lift (19”-24.5”) [140mm] | | Knee Tilt Mechanism   * Infinite Lock Free Float * Back Angle Adjustment * Adjustable Spring Tension * 2.5” Depth Adjustable Seat Slider   Base/Glides/Casters   * 25" Glass Reinforced Nylon High Profile Base * 5 Dual Wheel Nylon Carpet Casters   **Options:**   * 2 ¼” Glides [2G] * Chrome Accent Casters [CAC] * 26” Polished Aluminum Base [PB] * Single Wheel Casters [SW] * Single Wheel Urethane Casters [SWU] * Urethane Casters [UC] * 26” Glass Reinforced Nylon Base [26NB] * 26” Glass Reinforced High Profile Nylon Base [26HP2]   Additional Options   * Memory Foam Seat (Not Available on airCentric seat options) [EA] * Cal. 133 [Cal133] * Air Lumbar [AL] * Adjustable Headrest [AHRTS] | |