airCentric™2

|  |  |
| --- | --- |
| Knee Tilt | Midnight Black [air2-KT] |
|  |
| Backrest* 5" Patented Back Height Adjustment System
* Front Upholstered Dual Curve Backrest (19"w x 24"h)
* Plastic Back Cap with Airflow Vents
* Proprietary Airflow Molded Polyurethane Foam and Structure

Arms* [Click here](http://ergocentric.com/resource/arms) to view options

Seat* Tailored Upholstery on Seat Pan (20”w x 19”d)
* Proprietary Airflow Molded Polyurethane Foam and Structure

**Options:*** Extra Small (17.5”w x 15.5d) [XSS]
* Small Seat (18.5”w x 17”d) [SS]
* Plus Size (18.”w x 19”d) [PS]
* Extra Long Seat (20”w x 21”d) [XLS]
* Standard Seat (20”w x 19”d) [LS]
* Triple Density Foam (adds ¼” to seat width and depth) [TDF]

Pneumatic Lift (Seat Height)* 125 mm Pneumatic Lift (18" – 23")

**Options:*** 80 mm Pneumatic Lift (only available with 26” Glass Reinforced Nylon Base) (17.25”-20.25”) [80mm]
* 100 mm Pneumatic Lift (17.5”-21”) [100mm]
* 140 mm Pneumatic Lift (19”-24.5”) [140mm]
 | Knee Tilt Mechanism * Infinite Lock Free Float
* Back Angle Adjustment
* Adjustable Spring Tension
* 2.5” Depth Adjustable Seat Slider

Base/Glides/Casters* 25" Glass Reinforced Nylon High Profile Base
* 5 Dual Wheel Nylon Carpet Casters

**Options:*** 2 ¼” Glides [2G]
* Chrome Accent Casters [CAC]
* 26” Polished Aluminum Base [PB]
* Single Wheel Casters [SW]
* Single Wheel Urethane Casters [SWU]
* Urethane Casters [UC]
* 26” Glass Reinforced Nylon Base [26NB]
* 26” Glass Reinforced High Profile Nylon Base [26HP2]

Additional Options* Memory Foam Seat (Not Available on airCentric seat options) [EA]
* Cal. 133 [Cal133]
* Air Lumbar [AL]
* Adjustable Headrest [AHRTS]
 |