­­ergoCentricLittle Person Chair [ergo-LP]

|  |  |
| --- | --- |
| Backrest* Fully Upholstered Dual Curve Backrest (15.5” w x 13.5” h)

Arms* [Click here](http://w3.ergocentric.com/catalogue.asp?id=70) to view options

Seat* High Resilient Polyurethane Foam
* Seat Pan (15.75”w x 14”d)
* Eight Ply Hardwood Seat Structure

**Options:*** Small Seat (18.5"wx17"d) (Trigger Adjustable T-arms) [TATA] recommended with this option) [SS]
* Triple Density Foam Seat (Adds 1/4" to seat width and depth) [TDF]
* Tailored Upholstery on Seat Pan [TS]

Apt Control* Back Pivot and Seat Height

Pneumatic Lift (Seat Height)* 70 mm Pneumatic Lift (12" – 14.75")

**Options:*** 80 mm Pneumatic Lift (12.25" – 15.25")
* 100 mm Pneumatic Lift (12. 50" – 16")
* 140 mm Pneumatic Lift (14" - 18")
* 125 mm Pneumatic Lift (13” – 18”)
 | Base/Glides/Casters* 24" Glass Reinforced Nylon Base
* 26” Glass Reinforced Nylon Base (Upcharge)
* 5 Dual Wheel Nylon Carpet Casters 2

**Options:*** 2 ¼” Glides [2G]
* 26” Glass Reinforced Nylon Base [26NB]
* Single Wheel Casters [SW]
* Single Wheel Urethane Casters [SWU]
* Urethane Casters [UC]

Additional Options* 20" Diameter Height Adjustable Footring *(for use as a foot rest only)* [20FR]
* Back Trim [BT]
* Cal. 133 [Cal133]
* Boxed Weight/Size *(33 lbs/6.7 cu.ft)*

  |