tCentric Hybrid™

|  |  |
| --- | --- |
| Counter Height | Midnight Black [t-CH]  Light Grey [t-CHG] |
| Backrest:  Midnight Black / Light Grey   * Dual Curve Mesh Backrest (19"w x 25"h) * 5” Patented Back Height Adjustment System   Arms:  Midnight Black / Light Grey [G]  **Options:**   * tCentric Armrest Height & Lateral [TCL / TCLG] * tCentric Armrest Height & Swivel [TC360 / TC360G] * tCentric Armrest Height, Lateral & Swivel [TCL360 / TCL360G]   Seat:   * Dual Density Molded Polyurethane Foam * Eight ply hardwood seat structure * Tailored upholstery on seat pan (20”w x 19”d)   **Options:**   * Extra Small Seat (17 ½”w x 15 ½”d) [XSS] * Small Seat (18 ½”w x 17”d) [SS] * Plus Size Seat (22”w x 19”d) [PS] * Extra Long Seat (20”w x 21”d) [XLS] * Extra Deep Seat (22”w x 21”d) [XPS] * Energy Absorbent Memory Foam [EA] * Triple Density Foam [TDF] * Non-Tailored Seat Pan [NTS]   Pneumatic Lift (Seat Height):  Midnight Black / Light Grey   * 200 mm Pneumatic Lift (23 ½" – 30 ¾")   **Options:**  *Midnight Black / Light Grey [G]*   * 157 mm Pneumatic Lift (19 ¾” – 25 ½”) [157MM / G157MM] * 267 mm Pneumatic Lift (25 ¾” – 35 ¾”) [267MM / G267MM]   Measurements/Overall Dimensions:  Boxed Weight/Size: 56 lbs. / 6.7 cu.ft. | Counter Height Mechanism:   * Independent Back Angle Adjustment * Fixed Seat * Seat Height   **Options:**  *Midnight Black*   * Modified Multi Tilt Mechanism (Seat slider, height and back angle adjustment only) [MT] * Dedicated Task 2 Mechanism [DT2]   Base/Footring/Glides/Casters:   * 26" Glass Reinforced Nylon *(Midnight Black / Light Grey)* * Aluminum, Height Adjustable Footring (20” Diameter, 1 ¾” Thick Foot Platform) * 1 ¼” Glides   **Options:**   * Lock-On Urethane Casters [LON] * Lock-Off Urethane Casters [LOF] * Dual Wheel Nylon Casters [NC] * Dual Wheel Urethane Casters [UC] * Single Wheel Nylon Casters [SW] * Single Wheel Urethane Casters [SWU] * 2 ¼” Glides [2G]   Additional Options:  Midnight Black / Light Grey [G]   * Adjustable Headrest [AHR / AHRG]   \*Mixing of Midnight Black & Light Grey components is not an option. |