tCentric Hybrid™ Synchro Glide [t-SG]

|  |  |
| --- | --- |
| Backrest* 5" Patented Back Height Adjustment System
* Dual Curve Mesh Backrest (19"w x 25"h)

Arms* TC Armrest Height & Lateral [TCL]
* TC Armrest Height & Swivel [TC360]
* TC Armrest Height, Lateral & Swivel [TCL360]

Seat* Mesh Seat with 30% Glass Filled Nylon Frame
* Airless Cushion Technology
* Seat Pan 21"w x 19"d

**Six upholstered seat sizes options:*** Extra Small (17.5w" x 15.5"d) [XSS]
* Small (18.5"w x 17"d) [AFSS]
* Standard (20"w x 19"d) [LS]
* Plus Size (22"w x 19"d) [PS]
* Extra Long Seat (20"w x 21"d) [XLS]
* Extra Deep (22"w x 21"d) [XPS]

Synchro Glide Mechanism* 2.5" Depth Adjustable Seat Slider
* Adjustable Spring Tension
* Free Float
* Independent Back Angle Adjustment
* Seat Tilt Lock Out
* Synchro 2:1 Ratio

Pneumatic Lift (Seat Height)* 125 mm Pneumatic Lift (18"-23")

**Options:*** 100 mm Pneumatic Lift (17.5"-21") *100mm*
* 140 mm Pneumatic Lift (19"-24.5") *140mm*
* 80 mm Pneumatic Lift (17.25"-20.25") *80mm*
* 100 mm Pneumatic Lift Chrome (17.5"-21") *100mmCH*
* 125 mm Pneumatic Lift Chrome (18"-23") *25mmCH*
* 140 mm Pneumatic Lift Chrome (19"-24.5") *140mmCH*
 | Base/Glides/Casters* 26" Glass Reinforced Nylon High Profile Base 2
* 5 Dual Wheel Nylon Carpet Casters 2

**Options:*** Chrome Accent Casters [CAC]
* 26" Polished Aluminum High Profile Base [PB2]
* Urethane Caster [UC2]

Additional Options* Adjustable Headrest [AHR]
* CooltoTouch Lumbar Support (12"w x 6"h) [TLS]
* CooltoTouch Lumbar Supportwith Air Lumbar [TLSAL]

Measurements/Overall DimensionsBoxed Weight (60.65 lbs.)Mesh MaterialBoth the tCentric Hybrid seat and backrest are made from elastomeric mesh with fill yarns made from polyester. When stretched, this material yields excellent load-bearing properties and resiliency, showing less than5% load-bearing losswhen tested according toBIFMA standards.To clean use mild householdor hospital detergents.  |